UH-60 CREW BRIEFING

1) VERIFY CURRENCY – 60 Days – RCM, 90 Days – NRCM.

2) EQUIPMENT – ID Tags, ALSE, Pubs.

3) MISSION BRIEF – DA Form 5484-R.

4) MISSION OVERVIEW.

5) ROUTE OF FLIGHT.

6) WEATHER:

a) Current, Forecast, Winds

b) Advisories, Watches, Warnings

c) Illumination Data (%, SS, MR, MS, SR, etc.)

d) Void Time

7) ANALYSIS OF AIRCRAFT:

a) Logbook/preflight deficiencies.

b) Performance Planning:

(1) Comparison of computed ETF/ATF with logbook.

(2) Recomputation of PPC if necessary.

(3) GO/NO-GO Data.

(4) Single engine capability – Min/Max SE IAS.

(5) Fuel for mission.

8) CREW STATIONS.

9) CREW DUTIES:

a) Pilot on the Controls (P*).

(1) Fly aircraft, primary focus outside if VMC, inside if IMC.

(2) Obstacle/hazard avoidance.

(3) Monitor systems and instruments.

(4) Monitor and transmit on assigned radios as directed by PC.

b) Pilot not on the Controls (P).

(1) Assist in traffic and obstacle avoidance.

(2) Tune radios and set transponder.

(3) Navigate – Map, Doppler, GPS.

(4) Copy clearances, ATIS, and other pertinent information.

(5) Cross check instruments and systems.

(6) Monitor and transmit on assigned radios as directed by PC.

(7) Read and complete checklist items as required.

(8) Set/adjust switches and systems as required.

(9) Announce when focused inside more than 2-3 seconds.

c) Crewchief, medic, and other assigned crewmembers.

(1) Clear aircraft and tail on turns, approaches, etc.

(2) Secure passengers and cargo.

(3) Assist in traffic and obstacle avoidance.

(4) Operate armament IAW ROE and PC guidance.

(5) Perform other duties assigned by the PC.

10) IN THE EVENT OF AN EMERGENCY:

a) P*

(1) Initiate Immediate Action Emergency Steps.

(2) Look for landing area.

b) P

(1) Analyze emergency.

(2) Perform emergency procedure IAW checklist.

(3) Assist P*.

(4) Make radio call.

(5) Remind to lock shoulder harnesses.

11) EMERGENCY EGRESS LINK UP POINT:

a) Crewchiefs meet at pilot’s door on their side.

b) Right seat go around front to left side.

c) Left seat go around front to right side.

d) Meet and decide where to go.

e) If fire is present proceed upwind (if safe).

f) If injured/unconscious:

(1) No fire/fumes – leave me there, wait for medics.

g) If aircraft is on – GET ME OUT!!!
h) START FIRST AID.

12) OBSERVATION SECTORS.

13) NVG CONSIDERATIONS:

a) Verify currency – 45 days – RCM, 60 days – NRCM.

b) Equipment:

(1) Aircraft modifications and light (searchlight required).

(2) Operational NVG’s.

(3) Operational helmet mount.

(4) Spare NVG battery (should be zero time).

(5) Counter balance weight (secured, could be missile).

(6) Flashilights/Supplemental lighting.

c) Aircraft lighting configurations.

d) Forced landings:

(1) NVG – Searchlight as required.

(2) Unaided – Landing light – on unless it degrades vision.

e) NVG failure procedures.

14) INADVERTANT IMC PROCEDURES.

a) A,H,T,A.

b) NVG’s up after aircraft is under control (if applicable).

c) Cockpit lighting – turn up to full bright (if applicable).

d) EMERGENCY CONDITION!!!

15) SPECIAL MISSION CONSIDERATIONS:

a) Lost commo procedures.

b) Aircraft requirements – Cargo hook, ESSS, HUD, etc.

16) FINAL AIRCRAFT WALKAROUND.

17) QUESTIONS AND ACKNOWLEDGEMENT OF BRIEFING.

